[bookmark: _Hlk198567959]INVITATION FOR QUOTATION
FOR CONSTRUCTION OF SHADE FOR MUSHROOM CULTIVATION

Quotation ID.: MANT/CO/SRIJAN/2026-27/10 				           Dated: 24.09.2026

Manbhum Ananda Ashram Nityananda Trust (MANT) invites sealed quotations / digital quotations from reputed and authorized suppliers for construction of a shade for mushroom cultivation at Balurghat, Dakshin Dinajpur District, under Project SRIJAN, supported by HDFC Bank Parivartan.

1. Item Details
	Sl. No.
	Item Description
	Quantity Required

	1
	Shade- 15 ft X 10 ft
	3 nos



2. Technical Specifications and Requirements
a. Size of each shade/room:
· Length: 15 ft
· Width: 10 ft
· Minimum height: 10 ft from the top/ground level, as applicable to the structure.
· The structure shall be constructed as a single-slope roof to facilitate proper drainage of rainwater.
b. Bamboo Framework:
· The complete structural framework shall be made using strong, straight, and good-quality bamboo suitable for the construction.
· Bamboo framing shall be provided around the entire perimeter of the room, including adequate vertical supports, horizontal members, and roof supports.
· Bamboo members shall be properly tied/jointed and firmly anchored to ensure stability and durability.
· The contractor shall ensure that the structure remains rigid and does not become unstable due to wind or normal weather conditions.
c. Roofing / Shade Cover
· The roof shall be covered using 25 mm tin roofing sheets of good quality.
· Roofing sheets shall be properly aligned and securely fixed to the bamboo framework.
· Adequate overlap shall be maintained between adjoining sheets to prevent rainwater leakage.
· The roof shall have a single slope with sufficient gradient for effective drainage.
Insulation Arrangement:
· Jute wood shall be provided at the base/supporting arrangement of the tin roofing to help maintain proper insulation and reduce direct heat transfer from the tin sheet.
· The insulation arrangement shall be securely fixed and shall cover the required roofing/supporting area adequately.
d. Green Net:
· The complete room shall be surrounded/enclosed with good-quality green shade net on all sides.
· The green net shall be properly fixed to the bamboo framework without loose or open sections.
· The net should provide adequate ventilation while reducing direct sunlight and maintaining a suitable environment for mushroom cultivation.
· The contractor shall ensure that the green net is properly stretched and secured.
e. GI Wire Protection
· A GI wire protective arrangement shall be provided around the outside base of the green-net enclosure.
· The GI wire protection shall extend up to approximately 4 ft in height from ground level.
· The arrangement shall be sufficiently strong and properly fixed to protect the green net from damage caused by animals, movement around the structure, and other external factors.
f. Foundation and Fixing
· All bamboo posts/supports shall be properly fixed/anchored at the ground to provide adequate structural stability.
· The contractor shall ensure proper tensioning, tying and fixing of bamboo members, green net, GI wire and roofing materials.
· Any additional minor materials required for complete installation, such as binding wire, rope, fasteners, nails, clamps, supports and other fixing materials, shall be included in the quoted rate unless specifically excluded in the quotation.

3. Submission of Quotation
a. The quotation must be submitted in a sealed envelope and dropped into the tender box at the SRIJAN Project office, BT Park, Power House, Balurghat- 733103
b. For Digital copy, email us at: mant.kolkata@gmail.com, CC to: acctsrijan@gmail.com; sourav@mant.org.in; and anirban@cphr-mant.in; clearly mentioning “FOR THE  __________ (specific item name) <space> Specifications – Quotation ID:, Dated:.” 
c. Kindly note that mentioning and marking copies to all given email IDs during quotation submission is mandatory; otherwise, the quotation may be treated as invalid.
4. Important Dates
a. Last date for submission: 28th September, 2026
b. Opening of quotations: 29th September, 2026
c. Validity: All quoted rates should be valid for at least 60 days from the date of opening of the quotation. 
d. The purchase order will be issued within 3 days of the opening of the quotation, unless delayed by unforeseen circumstances.
e. Delivery Timeline: Within 20 days from the date of issue of the Purchase order. 
5. Contact Information
For any clarification, please e-mail: mant.kolkata@gmail.com / acctsrijan@gmail.com / anirban@cphr-mant.in / sourav@mant.org.in , Phone: +91-7044974566/ 6291565113. 

6. Terms & Conditions
a. MANT reserves the right to accept or reject any or all quotations without assigning any reason.
b. Technical responsiveness shall be assessed before commercial comparison. Procurement shall not necessarily be awarded to the lowest-priced quotation.
c. Any defective, damaged or improperly installed material/work shall be replaced or rectified by the supplier/contractor at no additional cost to MANT.
d. MANT reserves the right to increase or decrease the quantity of structures to be constructed.
e. Payment shall be made through RTGS/NEFT Bank Transfer only.
f. The quotation must bear the authorized signature and official seal of the supplier/contractor.
g. If the vendor is not previously registered with MANT, the prescribed Vendor Authentication/Registration Form along with the required documents must be submitted. MANT reserves the right to cancel the PO/order, even after issuance, and/or temporarily or permanently block the vendor in case of non-compliance or submission of false information.
h. The bidder shall clearly mention the unit rate per shade (15 ft × 10 ft), total rate for 4 shades, applicable taxes, transportation/installation charges, and any other applicable costs separately in the quotation. 
i. 2% TDS will be deducted for labour works as per the norms.


S/d
Dr. Nirmalya Mukherjee
Chief Executive
Manbhum Ananda Ashram Nityananda Trust (MANT)
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